# MOXA Power Input State Tool for DA Series

## Usage

```
USAGE:
        mx-input-power-state -i <power_port>

OPTIONS:
        -i <power_port>
                Get power input port state <connected/disconnected>

EXAMPLE:
        Get power input port 0 state
        mx-input-power-state -i 0
```

## Support Models

- DA series
  - DA-820E
  - DA-820C
  - DA-682C
  - DA-681C
  - DA-680
