Version Number: 3.0.1 
Product Line:   UPort 1200/1400/1600 Series Driver for Linux
Platform:       Linux kernel 3.x(x86/x64)
Company:        Moxa Inc.
Date:           2023/06/13

Support Product:
===============
UPort 1250, 1250I
UPort 1410, 1450, 1450I 
UPort 1610-8, 1650-8 
UPort 1610-16, 1650-16 

Tested Linux: 
=============
Kernel 3.7.10
Kernel 3.7.6
Kernel 3.5.1
Kernel 3.4.4
Kernel 3.2.0

Ubuntu 14.04 (3.13.0)
Ubuntu 12.10 (3.5.0)
Ubuntu 12.04 (3.2.0)
Ubuntu 11.0 (3.0.0)

Debian 7.8 (3.2.0)

Fedora 21 (3.17.4)
Fedora 19 (3.9.5)
Fedora 18 (3.6.10)

CentOS 7.4 (3.10)

SUSE 13.1 (3.11.6)
SUSE 12.3 (3.7.10)
SUSE 12.1 (3.1.0)

Release Note:
==============
Ver3.0.1
1. New: Support MUx50U UART.

Ver3.0
1. Improve: Support to disable FIFO by setserial utility.
2. Bugfix: Fix the issue that modem status is not correct after ports are
           opened.
3. Change: Divided an independent driver version 3.0 to support Linux kernel
           3.x.

Ver1.2
1. New: Support kernel version up to 3.4.4
2. Bugfix: Fix bug of compiling fail under gcc version 3.3.3. 
3. Bugfix: Fixed system memory leak when application keeps doing open/close 
           operations for a long time execution.
4. Bugfix: Fixed application hang up when open/close frequencytly.

Ver1.1
1. New: Support auto installation.

Ver1.0
1. New: Official released.

-End-
