Is it better to do the memory test with real allocation?

Make softboot configurable via watchdog.conf.

Test which applications are running.

RPC calls have to be taken from libtirpc to cope with their removal from glibc
2.14.

