Version Number: 6.0.1
Product Line:   MOXA UPort 1100 Series 
Platform:       Linux kernel 6.x(x86/x64/ARM32/ARM64)
Company:        Moxa Inc.
Date:           2024/02/15

Support Product:
================================
UPort 1110/1130/1130I/1150/1150I
USB Console

Latest Tested Linux Distribution: 
==================================
Fedora 37 (6.1.13)

Release Note:
===============================================================================
Ver6.0.1
1. Bugfix: Fix the compile error about "incompatible pointer type" for 
           break_ctl function return type in kernel 6.5.0.

Ver6.0
1. New: Divided an independent driver version 6.0 to support Linux kernel 6.x.

Ver5.1
1. New: Support ARM32/ARM64 platform.
2. Improve: Remove unnecessary source code.
3. Bugfix: Fix the compile error about "incompatible pointer type" for 
           get_serial function in struct usb_serial_driver in kernel 5.13.
Ver5.0
1. Improve: Supports Virtual Machine, ESXi v6.7.0. Tested guest OS is listed
            above.
2. Change: Divided an independent driver version 5.0 to support Linux kernel
           5.x.

Ver1.4
1. New: Add to support Moxa USB Console.
2. Improved: Support Linux kernel up to 4.x, which include RHEL 7 and CentOS 7
             (kernel 3.10.0). 
3. Bugfix: Eliminated compile-time message "error: implicit declaration of
           function 'signal_pending'" under kernel 4.11. 
4. Bugfix: Eliminated garbled text displayed when enabled Parity bit on an
           opened tty. 
5. Bugfix: Fix installation problem when using multiple UPort devices at the
           same time in kernel 3.11.
6. Change: No support for kernel 2.x. 

Ver1.3
1. Support kernel upto 3.4.4
2. Modify "mxu1_open" and "mxu1_close" function prototype.
3. Modify "mxu1_ioctl", "mxu1_tiocmget" and "mxu1_tiocmset" function prototype
4. Fix bug of DTR signal while setting baudrate to B0.

Ver1.2 
1. Add a new model UPort 1130I.
2. Support kernel upto 2.6.29
3. Fix bug of compiling fail on Kernel 2.6.24
4. Fix bug of compiling fail on FC 2 2.6.5 
5. Fix bug of installing driver with error -5 on 2.6.24.

Ver1.1
1. Add two new models UPort 1150, UPort 1150I.
2. Add static driver installation guide to the readme.txt.

Ver1.0
1. Official released.

-End-
