Version Number: 3.0.1
Product Line:   MOXA UPort 1100 Series 
Platform:       Linux kernel 3.x(x86/x64)
Company:        Moxa Inc.
Date:           2023/02/02

Support Product:
================================
UPort 1110/1130/1130I/1150/1150I
USB Console

Latest Tested Linux Distribution: 
==================================
CentOS 7.4
Debian 8.2
Fedora 20
openSUSE 13.2
Red Hat Enterprise Linux (RHEL) 7
Ubuntu 12.4 
Ubuntu 15.4

Latest Tested Linux Kernel:
============================
Kernel 3.19.0

Release Note:
===============================================================================
Ver3.0.1
1. Improve: Support "MOXA USB-to-Serial Port Driver" device.

Ver3.0
1. Change: Divided an independent driver version 3.0 to support Linux kernel
           3.x.

Ver1.4
1. New: Add to support Moxa USB Console.
2. Improved: Support Linux kernel up to 4.x, which include RHEL 7 and CentOS 7
             (kernel 3.10.0). 
3. Bugfix: Eliminated compile-time message "error: implicit declaration of
           function 'signal_pending'" under kernel 4.11. 
4. Bugfix: Eliminated garbled text displayed when enabled Parity bit on an
           opened tty. 
5. Bugfix: Fix installation problem when using multiple UPort devices at the
           same time in kernel 3.11.
6. Change: No support for kernel 2.x. 

Ver1.3
1. Support kernel upto 3.4.4
2. Modify "mxu1_open" and "mxu1_close" function prototype.
3. Modify "mxu1_ioctl", "mxu1_tiocmget" and "mxu1_tiocmset" function prototype
4. Fix bug of DTR signal while setting baudrate to B0.

Ver1.2 
1. Add a new model UPort 1130I.
2. Support kernel upto 2.6.29
3. Fix bug of compiling fail on Kernel 2.6.24
4. Fix bug of compiling fail on FC 2 2.6.5 
5. Fix bug of installing driver with error -5 on 2.6.24.

Ver1.1
1. Add two new models UPort 1150, UPort 1150I.
2. Add static driver installation guide to the readme.txt.

Ver1.0
1. Official released.

-End-
